|  |  |  |  |
| --- | --- | --- | --- |
| Date/Time | Facility | Severity | Message |
| Oct 22 17:45:59 | syslog | emerg | BCM96345 started: BusyBox v1.17.2  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: xDSL G.994 training  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 started  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 channel analysis  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: xDSL G.994 training  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: xDSL G.994 training  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 started  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 channel analysis  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 message exchange  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link up, interleaved, us=512, ds=6144  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: xDSL G.994 training  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 started  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 channel analysis  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link up, interleaved, us=512, ds=6144  |
| Oct 22 17:45:59 | daemon | alert | kernel: Intrusion -> IN=ppp0.1 OUT= MAC= SRC=132.255.32.15 DST=5.139.248.220 LEN=44 TOS=0x00 PREC=0x00 TTL=48 ID=13297 PROTO=TCP SPT=7210 DPT=23 WINDOW=51651 RES=0x00 SYN URGP=0 MARK=0x8000000  |
| Oct 22 17:45:59 | daemon | alert | kernel: Intrusion -> IN=ppp0.1 OUT= MAC= SRC=132.255.32.15 DST=5.139.248.220 LEN=44 TOS=0x00 PREC=0x00 TTL=48 ID=13297 PROTO=TCP SPT=7210 DPT=23 WINDOW=51651 RES=0x00 SYN URGP=0 MARK=0x8000000  |
| Oct 22 17:45:59 | daemon | alert | kernel: Intrusion -> IN=ppp0.1 OUT= MAC= SRC=116.109.36.234 DST=5.139.248.220 LEN=44 TOS=0x00 PREC=0x00 TTL=240 ID=6079 PROTO=TCP SPT=34888 DPT=23 WINDOW=14600 RES=0x00 SYN URGP=0 MARK=0x8000000  |
| Oct 22 17:45:59 | daemon | alert | kernel: Intrusion -> IN=ppp0.1 OUT= MAC= SRC=73.54.96.68 DST=5.139.248.220 LEN=40 TOS=0x00 PREC=0x00 TTL=50 ID=45970 PROTO=TCP SPT=24084 DPT=23 WINDOW=17676 RES=0x00 SYN URGP=0 MARK=0x8000000  |
| Oct 22 17:45:59 | daemon | alert | kernel: Intrusion -> IN=ppp0.1 OUT= MAC= SRC=132.255.32.15 DST=5.139.248.220 LEN=44 TOS=0x00 PREC=0x00 TTL=48 ID=13297 PROTO=TCP SPT=7210 DPT=23 WINDOW=51651 RES=0x00 SYN URGP=0 MARK=0x8000000  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: xDSL G.994 training  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 started  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: xDSL G.994 training  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 started  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 channel analysis  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 message exchange  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link up, interleaved, us=512, ds=736  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: xDSL G.994 training  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 started  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 channel analysis  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link up, interleaved, us=512, ds=6144  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: xDSL G.994 training  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 started  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 channel analysis  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link up, interleaved, us=512, ds=6144  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: xDSL G.994 training  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 started  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL G.992 channel analysis  |
| Oct 22 17:45:59 | daemon | crit | kernel: Line 0: ADSL link up, interleaved, us=512, ds=6144  |
| Oct 22 17:46:00 | daemon | crit | syslog: PPP LCP DOWN.  |
| Oct 22 17:46:00 | daemon | err | syslog: User name and password authentication failed.  |
| Oct 22 17:46:08 | daemon | crit | kernel: Line 0: ADSL link down  |
| Oct 22 17:46:10 | daemon | crit | kernel: Line 0: xDSL G.994 training  |

|  |
| --- |
|  |